# Scanner Configured as STX<BC>EOT
# Symbol LS 4071 Barcode Scanner
BarCode
	Read	\x02([^\x04]+)\x04
		String	Value[100] $1




