
STX	\x01%03u\a

ETX	%05u\c(2,0,1,-1)\x04

InfoA
	Poll 0\x1d\x03
	Read 0\
		(%03d)\
		(%04d)\
		(%02d)\
		(%03d)\
		(%05d)\
		(%05d)\
		(%04d)\
		(%03d)\
		(%03d)\
		(%03d)\
		(%04d)\
		(%04d)\
		(%04d)\
		(%08d)\
		(%04d)\
		(%04d)\
		(%04d)\
		(%04d)\
		(%04d)\
		(%04d)\
		(%04d)\
		(%08d)\
		(%08d)\
		(%08d)\
		(%08d)\
		(%08d)\
		(%08d)\
		(%03d)\
		(\d)\
		\x1d
		Long EventCode		$1
		Long Generator		$2
		Long Rotor		$3
		Real WindSpeed		$4/10
		Real Production		$5/10
		Real Consumption	$6/10
		Real Cos		$7/100
		Long Volt1		$8
		Long Volt2		$9
		Long Volt3		$10
		Long Amp1		$11
		Long Amp2		$12
		Long Amp3		$13
		Real TotalProduction	$14/10
		Long Thyristor		$15
		Long GearBearing	$16
		Long GearOil		$17
		Long Generatorg		$18
		Long Generator_G	$19
		Long Ambient		$20
		Long Nacelle		$21
		Long TotalProductiont	$22
		Long TotalProduction_G	$23
		Long TotalConsumption	$24
		Long BrakingDown	$25
		Long Contactor_G	$26
		Long Contactor		$27
		Real Time		$28/10
		Long Status		$29
					
		
Error
	Poll	1\x1d\x03
	Read	1\
		(%012u)(.)(%03u)\
		(%012u)(.)(%03u)\
		(%012u)(.)(%03u)\
		(%012u)(.)(%03u)\
		(%012u)(.)(%03u)\
		(%012u)(.)(%03u)\
		(%012u)(.)(%03u)\
		(%012u)(.)(%03u)\
		(%012u)(.)(%03u)\
		(%012u)(.)(%03u)\
		(%012u)(.)(%03u)\
		(%012u)(.)(%03u)\
		\x1d
		String	Time1[16]	$1
		String	Status1[2]	$2
		Long	Code1		$3
		String	Time2[16]	$4
		String	Status2[2]	$5
		Long	Code2		$6
		String	Time3[16]	$7
		String	Status3[2]	$8
		Long	Code3		$9 
		String	Time4[16]	$10
		String	Status4[2]	$11
		Long	Code4		$12
		String	Time5[16]	$13
		String	Status5[2]	$14
		Long	Code5		$15
		String	Time6[16]	$16
		String	Status6[2]	$17
		Long	Code6		$18
		String	Time7[16]	$19
		String	Status7[2]	$20
		Long	Code7		$21
		String	Time8[16]	$22
		String	Status8[2]	$23
		Long	Code8		$24
		String	Time9[16]	$25
		String	Status9[2]	$26
		Long	Code9		$27
		String	Time10[16]	$28
		String	Status10[2]	$29
		Long	Code10		$30
		String	Time11[16]	$31
		String	Status11[2]	$32
		Long	Code11		$33
		String	Time12[16]	$34
		String	Status12[2]	$35
		Long	Code12		$36

TOI
	Poll	2\x1d\x03
	Read	2\
		(%012X)\
		(%08X)\
		\x1d
		Digital In[1,48]	$1
		Digital Out[1,32]	$2


InfoB
	Poll 5\x1d\x03
	Read 5\
		(%03d)\
		(%03d)\
		(%03d)\
		(%03d)\
		(%04d)\
		(%08d)\
		(%06d)\
		(%08d)\
		(%06d)\
		(%08d)\
		(%05d)\
		(%08d)\
		(%05d)\
		(%08d)\
		(%08d)\
		(%08d)\
		\x1d
		Real Frequency		$1/10
		Long Thyristor		$2
		Long GearBearing	$3
		Long Pressure		$4
		Long Nacellep		$5
		Long Pump		$6
		Real PumpTime		$7/10
		Long Caliber		$8
		Real CaliberTime	$9/10
		Long YawCW		$10
		Real YawCWTime		$11/10
		Long YawCCW		$12
		Real YawCCWTime		$13/10
		Real OilPumpTime	$14/10
		Real NacelleFanTime	$15/10
		Real WaterPumpTime	$16/10


Production
	Poll 6\x1d\x03
	Read 6\
		(%08d)\
		(%08d)\
		(%06d)\
		(%08d)\
		\x1d
		Real Productiont	$1/10
		Real Consumptiont	$2/10
		Long WTG		$3
		Real WindDistance	$4/10

Start
	Write 3\x1d\x03
	Word Mode 

Stop
	Write 4\x1d\x03
	Word Mode 





